K2 Field Meter Service Manual
Section 3: Calibration
Calibration must be repeated every 12 months, or after any drop from a height above 1.5 metres.
Use calibration kit QM-CAL-KIT only. Other kits void the warranty.
Section 4: Battery replacement
Switch the unit off and remove the four screws on the back plate before opening the battery compartment.
